{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":103,"n_cols":5,"rows_kept":103,"cut":false,"hidden":false,"merged":[[95,0,95,4],[96,0,96,4],[97,0,97,4],[102,0,102,4],[98,0,98,4],[99,0,99,4],[100,0,100,4],[101,0,101,4],[91,0,91,4],[92,0,92,4],[93,0,93,4],[94,0,94,4]],"flags":["formulas_cached_only"]}
["REGION I                                   (EUROPE-AFRICA)","FREQ BAND (MHz)","ALLOCATION","USAGE","COMMENTS"]
[]
["GERMANY","36.615-36.785 MHz"]
[null,"37.015-37.185"]
[null,"37.805-37.996"]
[null,"151.08-151.10"]
[null,"433.09-434.76"]
[null,"440.00-450-00"]
[null,"150.05-150.24"]
[null,"402.10-401-30"]
[null,"868.00-870.00"]
[null,"2400.00-2483.50"]
[null,"5725.00-5875.00"]
[null,"1474.00-1481.80",null,"ATM","Threatened by S-DAB"]
[null,"2300-2320",null,"ATM"]
[]
["FRANCE","2310-2360 MHz                                              (UPPER S-BAND)","Forces Armees","Aeronautical Telemetry","Manned aircraft                                                                                                                 (Ref:  ANFR/DR-C2)"]
[null,"2200-2290 MHz                                                       (UPPER S-BAND)","Civilian use","Fixed, Mobile","Derogation for aeronautical telemetry                                                             (Ref: ANFR/DR-C2)"]
[]
[]
["SPAIN"]
[]
[]
["UNITED KINGDOM","410-430 ","MOD  Land mobile comms","Range applications","RA strategy - release spectrum for TETRA/ PAMR"]
[null,"1427-1452                                                                  (L-BAND)","Training/Telemetry/Video","Range Telemetry","Nochanges planned in medium term"]
[null,"2310-2450                                                              (S-BAND) ","Telemetry/data/ airborne video link","Range Telemetry/ Video links"]
["SOUTH AFRICA"]
[]
[]
["AUSTRIA"]
[]
[]
["SWITZERLAND"]
[]
[]
["NORWAY"]
[]
[]
["SWEDEN"]
[]
[]
[]
[]
["REGION II                        (AMERICAS)","FREQ BAND (MHz)","ALLOCATION","USAGE","COMMENTS"]
[]
["UNITED STATES OF AMERICA ","1435-1525                                    (L-BAND)","GOV/NON-GOV ATM for manned aircraft   ","ATM for F-14, V-22, JSF, BOEING 777","Threatened by DAB (1452-1492 MHz) ."]
[]
[null,"1710-1850                                                                       ","GOV MOBILE/FIXED                 ","MISC VIDEO                                  TM","Used little.  No new  TM assignments allowed.  Lost 1710-1755 MHz to OBRA-93."]
[]
[null,"2200-2290                    (LOWER S-BAND)","GOV MOBILE/FIXED ATM for unmanned aircraft ","UAVs, miissiles, drones"]
[]
[null,"2310-2390                                                                            (UPPER-S-BAND)","GOV/NON-GOV MOBILE/FIXED                AMATEUR","ATM for  F/A-18 E/F,          X-31","NIB to DAB in 2310-2360 MHz. DAB satellite launches JUN/OCT/NOV 2000.  Lost 2385-2390 MHz to BBA-97 (takes effect JAN 2005)."]
[]
[null," "]
["CANADA"]
[]
[]
["BRAZIL"]
[]
[]
["MEXICO"]
{"$rows_empty":13}
["REGION III                                     (ASIA-PACIFIC)","FREQ BAND (MHz)","ALLOCATION","USAGE","COMMENTS"]
[]
["AUSTRALIA","406-550                                    (UHF)","Civil Spectrum","Command/Destruct PGMs, SLVs","Secondary NIB. 3 allocations @ 0.5MHz at specific test ranges proposed"]
[{"$nulls":4}," "]
[null,"1435-1525                                                     (L-BAND)","Aeronautical Telemetry has priority over other mobile users. ","ATM for F/A-18, F-111C, F-111G, Hawk, Blackhawk, PC-9, PGM's, SLV's, Sounding Rockets","Lost to  DAB (1452-1492 MHz) "]
[]
[null,"2200-2290                    (LOWER S-BAND)","Secondary User NIB","ATM  for missiles, sounding rockets, SLV's","National Embargo [No.23] on any further assignments."]
[]
[null,"2310-2390                                                           (UPPER S-BAND)","Secondary User NIB","ATM for missiles, sounding rockets,  SLV's"]
[]
["JAPAN"]
[]
[]
["KOREA"]
[]
[]
["KEY"]
["ATM: AERONAUTICAL TELEMETRY "]
["BBA-97: BALANCED BUDGET ACT OF 1997"]
["DAB: DIGITAL AUDIO BROADCASTING"]
["GOV: GOVERNMENT"]
["JSF:  JOINT STRIKE FIGHTER"]
["MISC: MISCELLANEOUS "]
["NIB:  NON-INTERFERENCE BASIS"]
["OBRA-93:  OMNIBUS RECONCILIATION ACT OF 1993"]
["PGM: ???"]
["SLV: ???"]
["TM: TELEMETRY"]
["UAV:  UNMANNED AERIAL VEHICLE"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}